# GRAPHITE, FLUORINATED POLYMER CAS # 51311172

A Special Carcinogen E Dermal Hazard I Neurotoxin

B Human Terato\Repro Haz F Corrosive J Suspect Carcinogen

C Highly Toxic G Eye Damage K Suspect Terato\Repro Haz

D Inhalation Hazard H STEL L Sensitizers

HAZARD INDEX . . . . . . . . . . . .

NFPA HAZARD CODES (H,F,R,O) 0 0 0

ACUTE TOXICTY RISK INDEX 1.6 - LD50 12903.2 mg/Kg

INHALATION RISK INDEX <1 - LC50

ROUTE OF EXPOSURE

skin Contact: May cause skin irritation.

Eye Contact: May cause eye irritation.

Multiple Routes: May be harmful by inhalation, ingestion, or

skin absorption.

SIGNS AND SYMPTOMS OF EXPOSURE

To the best of our knowledge, the chemical, physical, and

toxicological properties have not been thoroughly investigated.

PHYSICAL CHARACTERISTICS

PHYSICAL STATE: Solid

SEGREGATION: SHELF # 2

STORAGE GROUP(S):

g - Non-Reactive/Non-Hazardous

WASTE CHARACTERISTIC HAZARD:

INCOMPATIBILITIES:Strong oxidizing agents.

FIRE EXTINGUISHER: Water spray. Carbon dioxide, dry chemical powder, or

appropriate foam.

TOXIC EMISSIONS WHEN BURNED: Hydrogen fluoride

REACTIVE PROPERTIES

HANDLING: Avoid inhalation. Do not get in eyes, on skin, on clothing.

STORAGE: Keep tightly closed. Store in a cool dry place.

The information presented in the OPMSDS is intended as a synopsis of relative hazard characteristics for this chemical, for application within the UMass-Boston Chem/XL Laboratory Program. This information is derived from a wide range of sources documented in that program. While these sources are considered credible, the user is cautioned that the university cannot guarantee the accuracy nor accept responsibility for damages which may arise from errors, omissions, or the use of this information in any context other than intended. The user is strongly encouraged to seek additional information whenever feasible.